RITTAL PDU Firmware V 5.15.xx
-----------------------------

IMPORTANT Information:
PDU firmware to work with DCIM Software RiZone !
As a RiZone user, ju must use this firmware version.
--

V5.15.40_2 (11.04.18) Rev. 847
Bugfix: Slow current measurement
Bugfix: Power display at idle speed
Change: Adjustment for manufacturing (1p chip)V5.15.40_2 (11.04.18) Rev. 847
--

V5.15.40  (19.09.17) Rev. 789
Bugfix: Update Charts on Mobile View

Bugfix: Libs adapted for radius

Bugfix: Switch-on behaviour relay at PoE
Feature: Upload Certificate
Feature: Dashboard
Feature: Mobile Website

Feature: Security Update - SSL, SSH, libcrypto

Feature: Email with TLS support

Feature: Sensors TMP / UNI / HUM / SEN Offset

Feature: Configuration history.

Feature: Charts for IE8

Feature: Modbus TCP

Feature: Status Simulation

Feature: Radius

Feature: Remote access for RiZone / sftp

Feature: partition description /docs/sysinfo.txt





- Based on CMC3 version 3.15.40



--
EOF


